Id;Default
53;Fan 2: Calibration error (InF)
54;Fan 2: Incorrect config. (CFF)
55;Fan 2: Invalid config. (CFI)
56;Fan 2: Modbus com. (SLF1)
57;Fan 2: Overcurrent (OCF)
58;Fan 2: Precharge (CrF1)
59;Fan 2: Drive overheat (OHF)
60;Fan 2: Motor overload (OLF)
61;Fan 2: Overbraking (ObF)
62;Fan 2: Mains overvoltage (OSF)
63;Fan 2: 1 output phase loss (OPF1)
64;Fan 2: Input phase loss (PHF)
65;Fan 2: Undervoltage (USF)
66;Fan 2: Motor short circuit (SCF1)
67;Fan 2: Overspeed (SOF)
68;Fan 2: Auto-tuning  (tnF)
69;Fan 2: Rating error (InF1)
70;Fan 2: PWR Calib. (InF2)
71;Fan 2: Int.serial link (InF3)
72;Fan 2: Int.Mfg area (InF4)
73;Fan 2: Ground short circuit (SCF3)
74;Fan 2: 3 out phASE loss (OPF2)
75;Fan 2: SoMove com. (SLF2)
76;Fan 2: HMI com. (SLF3)
77;Fan 2: Internal- I measure (InF9)
78;Fan 2: Internal- th. sensor (InFb)
79;Fan 2: IGBT overheat (tJF)
80;Fan 2: IGBT short circuit (SCF4)
81;Fan 2: Motor short circuit (SCF5)
82;Fan 2: Internal- CPU  (InFE)
83;Fan 2: Invalid configuration (CFI2)
84;Fan 2: Pr.Underload.Flt (ULF)
85;Fan 2: Proc.Overload Flt (OLC)
86;Fan 2: PI Feedback (SPIF)
87;Fan 2: AI current lost fault(LFF1)
52;Fan 1: AI current lost fault(LFF1)
51;Fan 1: PI Feedback (SPIF)
50;Fan 1: Proc.Overload Flt (OLC)
49;Fan 1: Pr.Underload.Flt (ULF)
48;Fan 1: Invalid configuration (CFI2)
47;Fan 1: Internal- CPU  (InFE)
46;Fan 1: Motor short circuit (SCF5)
45;Fan 1: IGBT short circuit (SCF4)
44;Fan 1: IGBT overheat (tJF)
43;Fan 1: Internal- th. sensor (InFb)
42;Fan 1: Internal- I measure (InF9)
41;Fan 1: HMI com. (SLF3)
40;Fan 1: SoMove com. (SLF2)
39;Fan 1: 3 out phASE loss (OPF2)
38;Fan 1: Ground short circuit (SCF3)
37;Fan 1: Int.Mfg area (InF4)
36;Fan 1: Int.serial link (InF3)
35;Fan 1: PWR Calib. (InF2)
34;Fan 1: Rating error (InF1)
33;Fan 1: Auto-tuning  (tnF)
32;Fan 1: Overspeed (SOF)
31;Fan 1: Motor short circuit (SCF1)
30;Fan 1: Undervoltage (USF)
29;Fan 1: Input phase loss (PHF)
28;Fan 1: 1 output phase loss (OPF1)
27;Fan 1: Mains overvoltage (OSF)
26;Fan 1: Overbraking (ObF)
25;Fan 1: Motor overload (OLF)
24;Fan 1: Drive overheat (OHF)
23;Fan 1: Precharge (CrF1)
22;Fan 1: Overcurrent (OCF)
21;Fan 1: Modbus com. (SLF1)
20;Fan 1: Invalid config. (CFI)
19;Fan 1: Incorrect config. (CFF)
18;Fan 1: Calibration error (InF)
17;Ethernet Override
16;Ethernet not connected
15;Communication to Temperatur Sensor PaintStop Address 14
14;Communication to Temperatur Sensor Charcoal Address 13
13;Communication to Fan 2 : Address 3
12;Communication to Fan 1 : Address 2
11;Communication to Co2/Voc Sensor Out Address 15
10;Communication to Co2/Voc Sensor In Address 16
9;VOC exceed 40%
8;Fan 2 Fault
7;Fan 1 Fault
6;Temperatur below 0° Celcius
5;Temperatur above 30° Celcius
4;Humidity exceeds 70%
3;CO2 exceed 350 ppm
2;Air flow less than 1800 m3/h
1;Dif press exceeds than 200pa
0;Dif press lower than 20pa
;
